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Institute reference. Match these component values to your board revision.
Refer to the schematic and layout in Figures 1 and 2 while assembling the LNA.
Assembly
Assemble all surface mount passives first: resistors, capacitors, and inductors. Work from left to right on the board. Install components with the same value together.
	Component Label
	Value

	L2
	10 nH

	L1, L3, L4, L5, L6
	100 nH

	C6
	9.1 pF

	C1, C5
	27 pF

	C15
	6.8 pF

	C4
	4700 pF

	C2, C3, C7, C8, C9, C10, C11, C12, C13, C14
	330 pF

	R5
	4.7k Ω

	R2
	27k Ω

	R1
	33k Ω

	R3
	50 Ω

	R8
	150 Ω

	R4, R13
	43 Ω

	R6
	17.4 Ω

	R7, R14
	5.8 Ω

	R9, R10
	287 Ω

	R11, R12, R15, R16
	870 Ω


Now place the actives:
	Component label
	Value
	Notes

	U2
	SAV-541
	Make sure the large pad lines up with the big foot

	U1, U3
	GALI-39+
	

	U4, U5
	BFCN-1445
	Align dot to point towards input

	IC1
	LM2940
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Figure 1: LNA circuit schematic
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Figure 2: LNA board layout
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