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In this activity you will use your multiple waveform signal source from Lesson 2 and add different types of  filters to see their effect on the output. 
Low-Pass Filter
Ideally, a low-pass filter allows signals with frequencies from 0 Hz to the "cutoff" frequency to pass through  unchanged, and it chops out signals above the cutoff frequency. You can think of it as a multiplier function  that multiplies the signal by 1 for signals below the cutoff frequency, and multiplies by 0 for signals above  the cutoff frequency. An analogy with liquids would be how a coffee filter works, allowing particles smaller  than a certain size to pass through, and particles greater than a certain size are filtered out and don’t pass  through.  
Real filters are unable to suddenly cutoff a signal from a multiplier of 1 to a multiplier of 0 at a single  frequency. The range of frequencies over which the multiplier changes from 1 to 0 is defined by the  transition width, as illustrated below: 
[image: ]
  Open your 6 function signal generator from Lesson 2. 
  Save as . . .  using a new file name. 
  Add a Low Pass Filter block to the canvas, and connect it after the Add block. 
  Open this block and change the FIR type to "Float → Float (Decimating)". This block should look  like the following: 
[image: ]
  Start with a Cutoff Freq of 1000 and a Transition Width of 50. The frequency values are in Hz. 
  Run the program. Adjust the frequencies of the signal sources, with some above and some below the  cutoff frequency. 
The frequency graph uses a logarithmic decibel (dB) scale. A 20 dB drop reduces amplitude to 1/10. A signal at -40 dB has 1/100 the amplitude of a signal at 0 dB.
  The Time Domain graph might be more convincing. Set several of the frequencies below the cutoff  frequency. Then increase them one by one to values way above the cutoff frequency. When only one  signal remains with a frequency below the cutoff, the time graph should look like a single sinusoidal  graph at that frequency. 
  Explore different Cutoff Freq’s and Transition Widths as well as different source frequencies. 
  Does the output behave as you would expect according to the simple model of a low-pass filter? 
High-Pass Filter
Ideally, a high-pass filter allows signals with frequencies above the cutoff frequency to pass through  unchanged, and it chops out signals below the cutoff frequency. As with a low-pass filter, there is also a  transition width associated with a real high-pass filter. A schematic diagram of the profile of a high-pass filter  is illustrated below: 
[image: ]
  Replace the Low Pass Filter with a High Pass Filter block. 
  Explore different Cutoff Freq’s and Transition Widths as well as different source frequencies, similar  to what you did for the low-pass filter. 
  Does the output behave as you would expect according to the simple model of a high-pass filter? 
Band-Pass Filter
Ideally, a band-pass filter allows signals with frequencies above the “low cutoff” frequency to pass through  unchanged, and it chops out signals above the high cutoff frequency. A schematic diagram of the profile of an  ideal high-pass filter is illustrated below: 
[image: ]
  Real band-pass filters have transition widths, as discussed with the other filters above. 
  Replace the High Pass Filter with a Band Pass Filter block. 
  Explore different Cutoff Freq’s and Transition Widths as well as different source frequencies, similar  to what you did for the other filters. 
In general, filters are used extensively in DSP. For instance, a spectrometer might be designed to detect a  certain frequency range. An appropriate band-pass filter could be used to remove much of the noise occuring  at frequencies above and below the desired range. 
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